RT\_Android\_Bluetooth\_SDK Demo Manual

1. Brief Introduction

RT\_Android\_Bluetooth\_SDK is a software development kit, which is for its

Android users to have their secondary development. It communicates with printer by bluetooth.

2. Function of SDK System

RT\_Android\_Bluetooth\_SDK supply integrated mobile printing, including blue tooth connection, character printing and image printing, Barcode printing and offering multiple printing functions, which covers most customers’ demand. Its character print support Double width, Double height, Underline, Small font, Bold and Reverse Type. Android programmer can find it convenient to reengineer through reading development document of RT\_Android\_Bluetooth\_SDK and referring to Demo of RT\_Android\_Bluetooth\_SDK.

3. Introduction of RT\_Android\_Bluetooth\_SDK

3.1. Software package

com.RT\_Printer.BluetoothPrinter.BLUETOOTH

3.2. Class

|  |  |
| --- | --- |
| Class Name | Discription |
| BluetoothPrintDriver | Bluetooth connection and printer cooperation |

For more details, please check the development document of RT\_Android\_Bluetooth\_SDK

4. SDK application illustration

An Android’s development environment, that is JDK+Eclipse+Android SDK, should be firstly established, before using this SDKs. After successful establishment, choose "Propertise" in the right-click menu of Project in Application. In the submenu of ＂Libraries＂--＂Java Build Path＂, choose ＂Add External JARs...＂to add＂ RT\_Android\_Bluetooth\_SDK.jar.＂in application program,then add as following:

**Import** com.RT\_Printer.BluetoothPrinter.BLUETOOTH.BluetoothPrintDriver;

5. RT\_Android\_Bluetooth\_SDK Demo’s Direction for Use


* 1. Installing Demo

Copy *BluetoothPrinter.apk* to the SD card of mobile phone or PAD that carried Android, open the document and install it. After that, logo could be found in the application program in the phone or PAD.




* 1. The instruction of Demo and its operation interface

Click the Bluetooth logo to start Demo, then operation interface will be the same as follow in Picture 1:



Picture 1 The operation interface after start

Click to connect the Bluetooth. Scan the around Bluetooth printer and try to connect the paired device one. Pls check as below Picture 2:





Picture 2 Connecting and scanning

Click ＂Scan＂ Device to add new device to the list. Click the paired device, it will connect directly and if not the paired ones, then there will show a dialog box, which ask you to pair fist. Input 0000 to the dialog box then the printer and phone will connect automatically after successful matching.

Printing could be started through phone or PAD after successful connection. Input what you want to print and click ＂*print＂*, then the input will be printed out. Also printing mode can be changed via choosing Double width, Double height ,Underline, Small font, Bold and Highlight.


Click ＂Inquiry Status＂to Check the battery voltage and the real-time printer status. Pls check as below Picture 3 and Picture 4:



Picture 3 Inquiry-no error Picture 4 Inquiry-no paper

Click ＂Test ＂to print the self-test page

Click ＂Pint Option＂, interface will be as Picture 5



Picture 5 Print options interface

Several printing function could be found in printing option.

Click ＂Print Text＂to print text．

Click ＂Print Picture＂ to print pictures．

Input barcode commands you need click ＂Print Barcode＂ to print it．

Click *＂*Print Receipt＂ to print the restaurant receipts

Click ＂Print Table＂to print express table

Click ＂Back＂ to returen to the main page．